**ANNEX II + III:TECHNICAL SPECIFICATIONS + TECHNICAL OFFER**

**Contract title: Supply of Patrol Clothing and Protective Work Clothing to EUMM Georgia**

**Contract reference number: EUMM-23-8479**

**Column 1-2 should be completed by the Contracting Authority**

**Column 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the Contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the Contracting Authority shows the required specifications (not to be modified by the tenderer).
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words “compliant” or “yes” are not sufficient).
* Column 4 allows the tenderer to make comments on its proposed supply and to make references to any eventual supporting documentation provided.
* **All columns of the Appendix 1 to the technical specifications are also to be filled in by the tenderer.**

Bids must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications. Bids that do not permit to identify precisely the type of products offered may be rejected by the evaluation committee.

**General requirements:**

Upon request tenderer must provide samples of items No 1.3 and No 1.4 to the EUMM.

|  |
| --- |
| **LOT 1: Patrol clothing and insignias with EUMM and EU flag logo** |

\* Pictures are for reference purpose only

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered** | | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| 1.1 | **Summer Cap with EUMM logo QTY: 150 pcs**  **Cap design:**  Baseball Cap with embroider EUMM logo front centre     * Material: Denim Cotton or equivalent natural fibres * Colour: Pantone Reflex Blue * Adjustable rear head strap * Min 3 air holes       **Logo**  EUMM logo centred on front of the cap     * Embroidered on cap * Design: see Annex A1 * Stars colour: Pantone Yellow * Text colour: White     *(example reference of logo front – not to be used as template* |  | |  |  |
| 1.2 | **Summer vest with EUMM logo QTY: 100 pcs**  Assorted sizes  Sized to fit over outer garments  **Vest design:**  For summer use   * Material: Cotton 50%/Polyester 50% +-5%; weight of 1sq.m >= 160 gr * Colour: Pantone Reflex Blue  Two lower front utility pockets with Velcro® closure: - One on each side   Length: 180 +/- 20 mm  Height: 200 +/- 20 mm  Width: 2 +/- 1mm * Two upper front utility pockets with Velcro® closure: - One on each side   Length: 110 +/- 10 mm  Height: 130 +/- 10 mm  Width: 2 +/- 1mm * Zipper closure – blue colour   Vest  **Logo front**  EUMM logo centred on the right side front upper most pocket   * Printed on vest * Design: see Annex A1 * Distance from star edge to star edge: 5 mm * Stars colour: Pantone Yellow * Text colour: White   Front logo  *(example reference of logo front – not to be used as template)*  **Logo back**  EUMM logo with text on back   * Printed on vest * Design: see Annex A1 * Distance from start to end point of lower text mass: 205 mm * Stars colour: Pantone Yellow * Text colour: White * Distance from top: 130 +/- 10 mm   Back logo  *(example reference of logo front – not to be used as template)* |  | |  |  |
| 1.3 | **Blue T-shirts for patrolling with printed EUMM logo and text QTY:140 pcs**  • **Sleeve:** short (just above the elbow).  • **Neck:** U  • **Fit:** box cut, relaxed fit  • **Colour:** EU Blue  • **Front side:** *EUMM surrounded by 12 stars* embroidered on the front. Colours: stars - pantone yellow, text – white (refer to Image 1.3.1 for guidance); area: 100x100 mm ± 5 mm.  • **Back side:** *European Union – 12 stars – Monitoring Mission* embroidered on the back side. Colours: stars - pantone yellow, text – white (refer to Image 1.3.2 for guidance); distance from top: 130mm ± 10 mm; distance from start to end point of lower text mass: 150 mm  • Fabrics and threads must be colour machine washing proof  • **Fabric:** 100% cotton or cotton/polyester mix up to 85/15 %  • **Fabric quality:** Cotton 170-180 g/6.0-6.3 oz. or equivalent for cotton/polyester mix  • Fabric must be pre-washed or pre-shrunk to avoid shrinking  • Each T-shirt must be packed individually in a transparent bag, with visible size label and EUMM neck label.  **Sizes:** Assorted male and female sizes. Size should be according to **joint European standard for size labelling of clothes** - **EN 13402 Size designation of clothes**  [https://en.wikipedia.org/wiki/Joint\_European\_standard\_for\_size\_labelling\_of\_clothes](https://eur06.safelinks.protection.outlook.com/?url=https%3A%2F%2Fen.wikipedia.org%2Fwiki%2FJoint_European_standard_for_size_labelling_of_clothes&data=05%7C01%7CAlexander.Kushashvili%40EUMM.EU%7C871cd90811f547acb02408dae418301c%7Ca8b768c05b61453e9b935ec9175e38b6%7C0%7C0%7C638073089776307698%7CUnknown%7CTWFpbGZsb3d8eyJWIjoiMC4wLjAwMDAiLCJQIjoiV2luMzIiLCJBTiI6Ik1haWwiLCJXVCI6Mn0%3D%7C3000%7C%7C%7C&sdata=V0YDVnxQAfqJXflZ4bV%2BMmJNCNVSrHWE2IPRHFb9HcM%3D&reserved=0)    **IMAGE 1.3.1**    **IMAGE 1.3.2** |  | |  |  |
| 1.4 | **Blue polo-shirts for patrolling with embroidered EUMM logo and text**  **QTY: 140 pcs**   * **Sleeve:** short (just above the elbow). On left sleeves max 150mm from top a Velcro attachment pad with a diameter of 80mm. * **Neck:** Casual with buttons * **Fit:** box cut, relaxed fit * **Colour:** EU Blue * **Front side:** *EUMM surrounded by 12 stars* embroidered on the front. Colours: stars - pantone yellow, text – white (refer to Image 1.4.1 for guidance); area: 100x100 mm ± 5 mm. * **Back side:** *European Union – 12 stars – Monitoring Mission* embroidered on the back side. Colours: stars - pantone yellow, text – white (refer to Image 1.4.2 for guidance); distance from top: 130mm ± 10 mm; distance from start to end point of lower text mass: 150 mm. * Fabrics and threads must be colour machine washing proof * **Fabric:** Knitted 100% cotton or cotton/polyester mix up to 80/20 % * **Feature:** Anti-wrinkle, QUICK DRY, compressed, breathable, sustainable material * **Fabric quality:** Cotton 190-220 g or equivalent for cotton/polyester mix * Fabric must be pre-washed or pre-shrunk to avoid shrinking * Each Polo-shirt must be packed individually in a transparent bag, with visible size label and EUMM neck label.   **Sizes:** Assorted male and female sizes. Size should be according to **joint European standard for size labelling of clothes** - **EN 13402 Size designation of clothes.**   * [https://en.wikipedia.org/wiki/Joint\_European\_standard\_for\_size\_labelling\_of\_clothes](https://eur06.safelinks.protection.outlook.com/?url=https%3A%2F%2Fen.wikipedia.org%2Fwiki%2FJoint_European_standard_for_size_labelling_of_clothes&data=05%7C01%7CAlexander.Kushashvili%40EUMM.EU%7C871cd90811f547acb02408dae418301c%7Ca8b768c05b61453e9b935ec9175e38b6%7C0%7C0%7C638073089776307698%7CUnknown%7CTWFpbGZsb3d8eyJWIjoiMC4wLjAwMDAiLCJQIjoiV2luMzIiLCJBTiI6Ik1haWwiLCJXVCI6Mn0%3D%7C3000%7C%7C%7C&sdata=V0YDVnxQAfqJXflZ4bV%2BMmJNCNVSrHWE2IPRHFb9HcM%3D&reserved=0)   Image 1 of Zegna embroidered logo polo shirt    **IMAGE 1.4.1**    **IMAGE 1.4.2** |  | |  |  |
| 1.5 | **Vest with EUMM logo reflective QTY: 100 pcs**  Sized to fit over outer garments  Assorted sizes  **Vest design:**  Dyna Med EMS Utility Vest or equivalent   * Material: 100% Polyester * Colour: Pantone Reflex Blue * One reflective stripe in the back:  - Height: 50 +/- 5 mm - Width: to fit vest size (covering the whole width of the vest) - 150 +/- 20 mm from the bottom of the vest.      * Two white reflective stripes on front on each half side of the vest: - One above upper right side utility pocket  - One above left side radio holder - Height: 50 +/- 5 mm - Width: to fit vest size (covering the whole width of the vest) * Two white reflective stripes on front lower right and left side utility pocket: - Covering the full length of each pocket - Height: 50 +/- 5 mm - Width: to fit vest size (covering the whole width of the pocket)      * Five front utility pockets with Velcro® closure: - All pockets on all sides aligned towards zipper - One lower left side and one lower right side  Width: 200 +/- 20 mm  Height: 140 +/- 20 mm - One above lower left side pocket and one above   lower right side pocket  Width: 170 +/- 10 mm  Height: 100 mm +/- 10 mm - One upper right side  Width: 130 +/- 10 mm  Height: 130 +/- 10 mm  With opening for pen/pencil on left side of flap * Zipper closure – black colour * Radio pocket on left chest with Velcro® antenna holder  **(should be able to carry a handheld radio Motorola DP4000/DP4000e with antenna and battery)** * 3 adjusting stripes on each side Type of desired adjusting stripe:   Washable in conventional washing machine  **Logo front**  EUMM logo centred on the right side front upper most pocket   * Printed on vest * Design: see Annex A1 * Distance from star edge to star edge: 75 mm (see attached electronic templates – Annex A2) * Stars colour: Pantone Yellow * Text colour: White   *(example reference of logo front – not to be used as template)*  **Logo back**  EUMM logo with text on back   * Printed on vest * Design: see Annex A1 * Distance from start to end point of lower text mass: 205 mm (see attached electronic templates – Annex A2) * Stars colour: Pantone Yellow * Text colour: White * Distance from top: 130 +/- 10 mm   *(example reference of logo front – not to be used as template)* |  | |  |  |
| 1.6 | **Beret with EUMM logo QTY: 25 pieces**  Assorted sizes  **Beret design:**  Beret should be one peace material/no stitching with EUMM Logo badge/ patch centred over the left eye   * Beret material: min 80% wool * Lace material: leather or artificial leather * Colour: Pantone Reflex Blue * Lining material: Cotton or equivalent natural fibres * two side mounted air holes * headband string, adjustable   **Badge/Patch design:**   * Shape: round * Diameter: 45mm – 50 mm * Embroidered EUMM Logo     **Logo**   * Design: see Annex A1 * Stars colour: Pantone Yellow * Text colour: White     *(example reference of logo front – not to be used as template* |  | |  |  |
| 1.7 | **Winter beanie with EUMM Logo QTY: 200 pcs**  **Beanie design:**  Knitted beanie with EUMM logo. Badge/Patch to be front centred on the inside of the Roll-over-Rim, upside down so when rolled-over it will be displayed correctly  External knitted fabric – Wool min 35%, polyester/ acrylic mix.  Lining material: Polar fleece (PET) or equivalent  Roll-Over Rim - min 60mm  Colour: Pantone Reflex Blue  Badge /Patch design: Shape: round  Diameter: 45mm – 50 mm  Colour; Pantone Reflex Blue  Embroidered EUMM Logo    **Logo**   * Design: see Annex A1 * Stars colour: Pantone Yellow * Text colour: White     *(Example reference of logo front – not to be used as template* |  | |  |  |
| 1.8 | **Summer Cap with EU flag logo QTY– 20 pcs**  **Cap design:**  Baseball Cap with printed EU flag logo front centre     * Material: Denim Cotton or equivalent natural fibres * Colour: Pantone Reflex Blue * Adjustable rear head strap * Min 3 air holes     **Logo**  EU flag logo centred on front of the cap     * Printed on cap * Stars colour: Pantone Yellow | |  |  |  |
| 1.9 | **Vest with EU flag logo reflective QTY: 20 pcs**  Sized to fit over outer garments  Assorted sizes  **Vest design:**  Dyna Med EMS Utility Vest or equivalent   * Material: 100% Polyester * Colour: Pantone Reflex Blue * One reflective stripe in the back:  - Height: 50 +/- 5 mm - Width: to fit vest size (covering the whole width of the vest) - 150 +/- 20 mm from the bottom of the vest. * Two white reflective stripes on front on each half side of the vest: - One above upper right side utility pocket  - One above left side radio holder - Height: 50 +/- 5 mm - Width: to fit vest size (covering the whole width of the vest) * Two white reflective stripes on front lower right and left side utility pocket: - Covering the full length of each pocket - Height: 50 +/- 5 mm - Width: to fit vest size (covering the whole width of the pocket) * Five front utility pockets with Velcro® closure: - All pockets on all sides aligned towards zipper - One lower left side and one lower right side  Width: 200 +/- 20 mm  Height: 140 +/- 20 mm - One above lower left side pocket and one above   lower right side pocket  Width: 170 +/- 10 mm  Height: 100 mm +/- 10 mm - One upper right side  Width: 130 +/- 10 mm  Height: 130 +/- 10 mm  With opening for pen/pencil on left side of flap * Zipper closure – black colour * Radio pocket on left chest with Velcro® antenna holder  **(should be able to carry a handheld radio Motorola DP4000/DP4000e with antenna and battery)** * 3 adjusting stripes on each side Type of desired adjusting stripe:   Washable in conventional washing machine  **Logo front**  EU Flag logo centred on the right side front upper most pocket   * Printed on vest * Distance from star edge to star edge: 75 mm * Stars colour: Pantone Yellow   **Logo back**  EU Flag logo on back   * Printed on vest * Stars colour: Pantone Yellow * Distance from top: 130 +/- 10 mm | |  |  |  |
| 1.10 | **Winter beanie with EU Flag Logo Qty: 20 pcs**  **Beanie design:**  Knitted beanie with EU Flag logo. Badge/Patch to be front centred on the inside of the Roll-over-Rim, upside down so when rolled-over it will be displayed correctly  External knitted fabric – Wool min 35%, polyester/ acrylic mix.  Lining material: Polar fleece (PET) or equivalent  Roll-Over Rim - min 60mm  Colour: Pantone Reflex Blue  Badge /Patch design: Shape: round  Diameter: 45mm – 50 mm  Colour; Pantone Reflex Blue  Embroidered EU Flag Logo  **Logo**   * Stars colour: Pantone Yellow | |  |  |  |

|  |
| --- |
| **LOT 2: New Design vest with EUMM logo reflective** |

\* Pictures are for reference purpose only

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| 2.1 | **New Design of Vest with EUMM logo reflective QTY: 200pcs**   * Multi-functional reflective safety vest or equivalent * **Material:** 400gsm double-layer polyester mesh fabric (refer to image 3.1 for guidance) * **Colour:** Pantone Reflex Blue (Fluorescent EU blue) * Lightweight design made with breathable fabrics * One reflective stripe in the back 150mm ± 20 mm from the bottom of the vest (refer to image 3.2 for guidance):  - Height: 50 mm ± 5 mm - Width: to fit vest size (covering the whole width of the vest) * Two white reflective stripes on front on each half side of the vest (refer to image 3.3 for guidance): - One above upper right side utility pocket  - One above left side radio holder - Height: 50 mm ± 5 mm - Width: to fit vest size (covering the whole width of the vest) * Two white reflective stripes on front lower right and left side utility pocket (refer to image 3.3 for guidance): - Covering the full length of each pocket - Height: 50 mm ± 5 mm - Width: to fit vest size (covering the whole width of the pocket) * Four front utility pockets with Velcro® closure (refer to image 5.3 for guidance): - All pockets on all sides aligned towards zipper - One lower left side and one lower right side  Width: 200 mm ± 20 mm  Height: 150 mm ± 20 mm - One above lower left side pocket and one above lower right side pocket  Width: 160 mm ± 10 mm  Height: 120 mm ± 10 mm - One upper right side  Width: 130 mm ± 10 mm  Height: 130 mm ± 10 mm  With opening for pen/pencil on left side of flap * Zipper closure: blue colour * The vest should be closed with Velcro® closure in the sides to ensure flexibility * Radio pocket on left shoulder with Velcro® antenna holder (refer to image 5.1 for guidance) **(should be able to carry a handheld radio Motorola DP4000/DP4000e with antenna and battery)** * Washable in conventional washing machine   **Logo front**  Velcro for logo on the right upper pocket flap in dimension 10x10cm  EUMM logo centred on the Left side front upper most pocket   * Printed on vest * Distance from star edge to star edge: 75 mm (see attached electronic templates – Annex A1) * Stars colour: pantone Yellow * Text colour: white * Printing must be wash machine proof and with reflex efforts.   refer to image 3.4 for guidance  *(example reference of logo front – not to be used as template)*  **Logo back**  On the upper part of the back a blue polyester fabric with Velcro for logo size 30x13cm should be prepared  EUMM logo with text on back   * Printed on vest * Distance from start to end point of lower text mass: 205 mm (see attached electronic templates – Annex A1) * Stars colour: pantone Yellow * Text colour: white * Distance from top: 130mm ± 10mm * Printing must be wash machine proof and with reflex efforts.   refer to image 3.5 for guidance.  *(example reference of logo back – not to be used as template)*  Final design and layout will be developed by the Contractor in conjunction with the Contracting Authority and finally approved by the Contracting Authority.    **IMAGE 3.1**    **IMAGE 3.2**    **IMAGE 3.3**    **IMAGE 3.4**    **IMAGE 3.5** |  |  |  |

|  |
| --- |
| **LOT 3: Personnel Protective clothing** |

\* Pictures are for reference purpose only

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| 3.1 | **Men’s waterproof pants: QTY: 25 pcs**  water resistant - treated with durable water repellent abrasion and tear resistant.  quick drying (Flash Dry XD technology or equivalent) belt loops and adjustable with partial elastic waistband or belt hand pockets and covered back pocket enhanced mobility due stretch fabric, crotch gusset and darting at knees weight 260 – 360 grams  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.2 | **Men’s insulated pants: QTY: 5 pcs**  waterproof - treated with durable water repellent, seam-sealed breathable:   * allows water vapors to pass through from inside to outside (DryVent™ 2L technology or equivalent) * preferably with zip inner-thigh vents   warmth retention even in wet weather (Heatseeker™ Eco technology or equivalent)  belt loops and adjustable waist with Velcro tabs  articulated knees reinforced kick patches and hem  secure-zip hand pockets inside gaiters with elastic to prevent snow from getting inside the pants  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.3 | **Men’s down jacket: QTY: 25 pcs**  2 or 3 in 1, composed of:   * outer shell combined with * an attached or removable hood and * a removable inner jacket   **the outer shell:**   * waterproof - treated with water repellent, sealed seams * windproof * breathable – allows water vapors to pass through from inside to outside (DryVent™ 2L technology or equivalent) * able to prevent condensation and sweat (preferably by pit venting with zip) * full zip front reverse coil zipper with storm flap * hook & loop neck closure * outside zip secured pockets (both sides and one on the chest) * adjustable wrist cuffs with Velcro tabs   **the hood:**   * attached or detachable from the outside shell * adjustable   **the inner jacket:**   * detachable from the outside shell by zip * wearable as standalone clothing * outside zip secured pockets (sides) * compressible and warmth retainer (minimum 500 fill goose down)   Weight: 850 - 1300 grams  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.4 | **Men’s trench (parka): QTY:25 pcs**  waterproof - treated with durable water repellent  windproof  breathable – allows water vapors to pass through from inside to outside (DryVent™ 2L technology or equivalent) attached hood, adjustable with drawcord insulated min. 550 fill Down  center front zip covered by draft flap with hook-and-loop closure  outside dual entry side pockets:   * top-entry hidden hook-and-loop flap closure * the side-entry with zip closure   inside zip secured chest pocket  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.5 | **Fleece jacket QTY: 5 pcs.**  water repellent - treated with durable water repellent windproof collar, shoulders, chest and lower-back sleeves preferably reinforced for abrasion resistance stretch fabric on cuffs for added mobility center front zip  outside zip secured pockets (both sides and one on the chest)  Weight: 450 - 600 gram  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.6 | **Winter gloves QTY: 25 pairs**  waterproof - treated with durable water repellent, windproof, adjustable wrist cuffs with Velcro tabs, 5 fingers, touchscreen compatible  silicone gripper palm insulated to provide extra warmth (Heatseeker™ Eco technology or equivalent)  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.7 | **Boots QTY: 25 pairs**  Waterprooffront rubber mudguard (preferably all around)insulated to provide extra warmth (ThermoBall™ Eco technology or equivalent)  comfortable footbed (OrthoLite® Eco LT™ technology or equivalent)outsole designed for good traction on snow and ice (UltrATAC™ technology or equivalent)upper waterproof leatherupper overlays to prevent snow from getting inside the boots  Weight: 500 - 600 gram  Height: 15 - 19 cm  Assorted sizes  Dark color - to be determined, based on offer |  |  |  |
| 3.8 | **Protective Jacket QTY: 9 pcs**   * Ripstop fabric * Multiple pockets * High collar * Central zipper with front flap * Velcro adjustable cuffs * Details of visibility * Stretch inserts for armholes * Longer back   Colour – dark grey/anthracite or similar dark shades  First product photo |  |  |  |
| 3.9 | **Protective pants QTY: 9 pcs**   * Elasticated waistband * Multiple pockets * Multiple tool loops * Knee pad pockets * Colour – dark grey/anthracite or similar dark shades   PPE category II  A picture containing clothing, person, suit, wearing  Description automatically generated |  |  |  |
| 3.10 | **Softshell jacket QTY: 9 pcs**   * Out shell >> Softshell (polyester / Spandex) * water resistance and breathable * micro polar fleece * full Zipper YKK * Elasticated cuffs with scratch bands Flap   Colour – dark grey/anthracite or similar darker shades to black  First product photo |  |  |  |
| 3.11 | **Jacket QTY: 9 pcs**   * Nylon Micro-Ripstop * mechanical stretch + TPU membrane + fleece * Chin guard * zipped patch chest pocket – desired * 2 vertical lower pockets + invisible zippers inserted in the seam * Longer back   Colour – dark grey/anthracite or similar darker shades to black  First product photo |  |  |  |
| 3.12 | **T-shirt** **QTY: 47 pcs**   * Polo type, short sleeves * Cotton (allowed additions in the fabric for better performance) * Anti-odour   Colour – dark grey/anthracite or similar darker shades to black  First product photo |  |  |  |
| 3.13 | **Protective boots QTY: 19 pairs**   * Reinforced toecap * Ant penetration textile sole * External sole in double density PU/PU * Upper in Suede * Non-woven lining, breathable * Padded collar * Footbridge supplying torsional rigidity * Midsole with front protective covering * PPE Category – II   Colour – (dark) grey/anthracite or similar darker shades to black  First product photo |  |  |  |
| 3.14 | **High visibility safety vest Qty: 9 pcs**  Reflective Vest Belt Jacket, Woven reflective elastic belt.  360 degrees visibility  One size fit all, adjustable to most sizes.  Reflector Strips  Amazon.com : Reflective Vest, Reflective Glow Belt with 2Pack Reflector  Armbands, Adjustable Elastic Safety Vest Outdoor Reflective Belt High  Visibility, Ultralight & Comfy for Running, Jogging, Walking, Cycling, :  Sports & Outdoors |  |  |  |
| 3.15 | **Protective gloves QTY: 9 pairs**   * Anti-impact TPR reinforcements on back of hand and fingers * Reinforced crotch between thumb and index * Reinforced palm with cushioning area * Neoprene wrist with Velcro fastening. * Fingertips of thumb, index and middle finger with integrated PU touchscreen grip – desired   PPE category – II |  |  |  |
| 3.16 | **Helmet QTY: 9 pcs**   * ABS Shell * 6 point textile suspension harness in polyester and LDPE cradle * Textile headband * 3-point chin strap in polyester   breaking strength between 15 and25 daN, |  |  |  |