# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

# Contract title: ****Framework contract for Supply and Delivery of Fuel for EUMM Vehicles & Generators****

**Publication reference: EUMM-23-8594**

**Column 1-2 should be completed by the Contracting Authority**

**Column 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the Contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the Contracting Authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words “compliant” or “yes” are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation Committee’s notes** |
| --- | --- | --- | --- | --- |
|  | Provision of Diesel fuel (with low sulphur content, less than 10 mg/kg, minimum cetane No 51) at the Contractor's distribution points especially at: **Zugdidi, Gori, Sachkhere, and Tbilisi** (with possibility of bulk fuel delivery to any of EUMM Locations). When applicable, winter type fuel with the fuel filter blocking temperature down to – 20 0C  Fuel specifications shall conform in all respects the requirements specified in **Annex II of the Directive 98/70/EC** of The European Parliament and af the Council,of 13 October 1998, **relating to the quality of petrol and diesel fuels** and amending Council Directive 93/12/EEC.  Quantity up to 260 000 l |  |  |  |
|  | Provision of Petrol fuel (with low sulphur content, less than 10 mg/kg, unleaded, minimum octane No 95) at the Contractor's distribution points especially at: **Zugdidi, Gori, Sachkhere, Mtskheta, and Tbilisi**.  Fuel specifications shall conform in all respects the requirements specified in **Annex I of the Directive 98/70/EC** of The European Parliament and af the Council,of 13 October 1998, **relating to the quality of petrol and diesel fuels** and amending Council Directive 93/12/EEC.  Quantity up to 35 000 l per year |  |  |  |
|  | Provision of an electronic fuel distribution system, with the following minimum requirements:   * web based access to the EUMM allocated by the supplier account, with proven online operations security * on when needed basis – electronic, online individual and bulk reports, over time-varying periods, to include: * Date and time of the refuelling * Location of the refuelling * Exact quantity of fuel type added to the EUMM vehicle’s fuel tank * EUMM vehicle mileage at the moment of refuelling (desired feature, the subject of system development status) * possibility of the reports export into Excel file * capability of each individual EUMM vehicle’s electronic fuel distribution mean for the online fuel add/remove operations * 24/7 access to the EUMM fuel account * all refuelling operations carried out with the online permanent and secure connection |  |  |  |
|  | Provision of Fuel cards (or any other electronic fuel distribution means) for all EUMM vehicles, free of charge, on when needed basis. |  |  |  |

To ensure full operational readiness of EUMM vehicle fleet it is foreseen to carry out independent fuel quality inspection at identified by EUMM fuel stations in accordance to EU fuel quality Directive.